CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2pl72/conf/instr/spect/uxnmr.info
Date         : Fri Jan 19 10:20:36 2024
Release      : TOPSPIN Version 3.2-pl7
Installed in : C:/Bruker/TopSpin3.2pl72
Host         : NMR1
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Core(TM) i5-4460 CPU @ 3.20GHz (4 cores at 3192 MHz)
User         : Administrator
Description  : Avance III 400
Location     : 
System       : Avance III NMR spectrometer
1H-frequency : 400.13 MHz
Order Number : 
Configured in: C:/Bruker/TopSpin3.2pl72/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : 1
- FREDs : none
- DPP : none

DRU: AQS DRU Z100977/00710 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 150604
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x72   0x3    AW  R  3.0 REC-1  AQS RXAD400 Z102116/861 ECL 03.00
     3   0x34  0x2   0x1        X  5.0 REF-1  REF-400 Reference Board for AQS Receiver
     4   0x24 0x11   0x8    AE  S  2.1 SGU-1  AQS SGU/2 400 Z103080/00644 ECL 02.01 FPGA-Vs=AF
     5   0x25 0x11   0x8    AE  S  2.1 SGU-2  AQS SGU/2 400 Z103080/00611 ECL 02.01 FPGA-Vs=AF
     9   0x36  0x5     0        A  6.0 BLA-1  BLA2BB 150/60 20-400 W1345049/1919 ECL 6
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  2.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS-Minirouter

Amplifiers (AQS configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        B      150    N         BLA2BB 150/60 20-400 W1345049/1919/-
   2      1         2        B       60    N         BLA2BB 150/60 20-400 W1345049/1919/-
   3      2         1       2H       20    N         2HTX in BSMS -/-/-


BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 20
- Shim System = BOSS1-SB
- 2HTX Amplifier: available
- Lock: installed

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty05
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty04

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AO
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H/2H 1H (virtual 50 Ohm reference: 281.1%/93.0deg)
                 PN=Z003959, SN=00481 from 20071008
    Module  2 : 1H/2H 2H (virtual 50 Ohm reference: 91.7%/-74.3deg)
                 PN=Z003959, SN=00481 from 20071008
    Module  3 : XBB19F 2HS
                 PN=Z003504, SN=00477 from 20071015


Frequency generation:
- F1: for SGU
- F2: for SGU



RF cable connections (assumed)
--------------------------------------------------------------------
SGU1 NORM output -> input 2 of transmitter 1 (BLA2BB 150/60 20-400 W1345049/1919)
SGU1 AUX  output -> input 1 of transmitter 2 (2HTX in BSMS)
SGU2 NORM output -> input 3 of transmitter 1 (BLA2BB 150/60 20-400 W1345049/1919)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (assumed)
--------------------------------------------------------------------
transmitter 1 (BLA2BB 150/60 20-400 W1345049/1919) amplifier B-150W uses blanking 1
transmitter 1 (BLA2BB 150/60 20-400 W1345049/1919) amplifier B-60W uses blanking 2
transmitter 2 (2HTX in BSMS) amplifier 2H-20W uses blanking 3

